|  |
| --- |
|  |
| Configuring iLO 4 |
|  |
|  |
|  |
|  |

|  |
| --- |
|  |

Configuring a static iLO IP address by using iLO RBSU

To configure a static IP address for the iLO interface:

1. Restart or power on the server.
2. Press **F8** in the HP ProLiant POST screen.

The iLO RBSU screen appears.

1. Disable DHCP:  
   1. Select **Network 🡺 DNS/DHCP**, and then press **Enter**.

The **Network Autoconfiguration** window opens.

* 1. Select **DHCP Enable**, as shown in below figure

* 1. Press the spacebar to set **DHCP Enable** to **OFF**, and then press **F10** to save the changes.

1. Enter an IP address and subnet mask:  
   1. Select Network **🡺** **NIC and TCP/IP**, and then press **Enter**.

The **Network Configuration** window opens.

* 1. Enter the appropriate information in the **IP Address, Subnet Mask**, and **Gateway IP Address** fields, as shown in below figure:  
       
     
  2. Press **F10** to save the changes

1. Select **File** **🡺** **Exit** to exit iLO RBSU.

The changes take effect when you exit iLO RBSU.

Adding iLO user accounts by using iLO RBSU

To add local iLO user accounts:

1. Restart or power on the server.
2. Press **F8** in the HP ProLiant POST screen.

iLO RBSU starts.

1. Select **User** **🡺 Add**, and then press **Enter**.
2. The **Add User** screen appears, as shown in below figure:  
     
   

1. Enter the following user account details:
   1. User name
   2. Login name
   3. Password and Verify Password
2. Ensure that all the iLO privileges are enabled by setting them to **Yes**.
   1. **Administer User Accounts** **🡺 Yes**
   2. **Remote Console Access** **🡺 Yes**
   3. **Virtual Power and Reset** **🡺 Yes**
   4. **Virtual Media** **🡺 Yes**
   5. **Configure iLO Settings** **🡺 Yes**
3. Press **F10** to save the new user account.
4. Select **File** **🡺 Exit** to exit iLO RBSU.